# ID 50403

Probe already actuated.
Description | The edge banding function checks whether the measuring probe is already enabled before starting the edge banding motion. The signal may not be enabled. For more information on edge banding, see [PROG// Section: Edge banding (G108)].
Response | Class | 4 | Motion stop, abort edge banding.
Solution | Class | 6 | Check measurement signal and signal level.
Parameter | %1: | Logical axis number [-]
Logical axis number of axis affected P-AXIS-00016.
Error type | 1, Error message from NC program.