# Reduced maximum acceleration (P-AXIS-00545)

P-AXIS-00545 | Reduced maximum acceleration for manual operation without parallel interpolation
Description | The parameter defines the active acceleration for manual mode with an active PLC control signal via the control unit Activation of reduced manual mode acceleration (bahn_mc_control.reduced_acceleration).
Parameter | handbetrieb.hb.a_max_red
Data type | UNS32
Data range | 0 < a_max_red ≤ P-AXIS-00008
Axis types | T, R
Dimension | T: mm/s² | R: °/s²
Default value | 1000
drive types. | ----
Remarks |