# Overview

Constant | Description
--- | ---
SLOPE_VB_MAX | Maximum axis speed that can be parameterised
ACHS_NAME_LAENGE | Maximum length of the axis designation

ID | Parameter | Description
--- | --- | ---
P-CHAN-00082 | spdl_anzahl | Number of spindles in the channel
P-CHAN-00036 | log_achs_nr | Spindle axis number
P-CHAN-00007 | bezeichnung | Spindle designation
P-CHAN-00010 | default_ax_name_of_spindle | Name of the spindle as channel axis
P-CHAN-00043 | m19_synch | Synchronisation type of the M19 function
P-CHAN-00045 | m3_synch | Synchronisation type of the M03 function
P-CHAN-00047 | m4_synch | Synchronisation type of the M04 function
P-CHAN-00049 | m5_synch | Synchronisation type of the M05 function
P-CHAN-00081 | s_synch | Synchronisation method of the S function
P-CHAN-00051 | main_spindle_ax_nr | Definition of Main Spindle
P-CHAN-00052 | main_spindle_gear_change | Enabling gear changes
P-CHAN-00053 | main_spindle_name | Main spindle designation
P-CHAN-00074 | range_way | Search direction in the speed range table
P-CHAN-00004 | autom_range | Automatic gear speed change
P-CHAN-00058 | range_table[j].min_speed | Lower limit of speed ranges
P-CHAN-00055 | range_table[j].max_speed | Upper limit of speed ranges
P-CHAN-00008 | cax_face_id | Face machining variant (turning/milling)
P-CHAN-00094 | kinematik[i].param[j] | Kinematic offsets for face/lateral surface machining up to Build V3.00
P-CHAN-00262 | trafo[j].id | Kinematics ID of lateral surface machining
P-CHAN-00263 | trafo[j].param[k] | Kinematic offsets for face/lateral surface machining as of Build V3.00
P-CHAN-00761 | tapping.use_actual_position | Tapping with actual positions of the spindle
P-CHAN-00762 | tapping.n_cycles | Number of filter cycles to filter actual spindle positions

ID | Parameter | Description
--- | --- | ---
P-AXIS-00015 | achs_mode | Axis mode
P-AXIS-00016 | achs_nr | axis number
P-AXIS-00018 | achs_typ | Axis type
P-AXIS-00058 | durchm_prog_abs | Diameter programming (G51) at G90.
P-AXIS-00059 | durchm_prog_rel | Diameter programming (G51) at G91.
P-AXIS-00220 | vb_regelgrenze | Limit velocity of the measuring system
P-AXIS-00216 | vb_min_null | Limit value for speed 0