# ID 21493

Value for the maximum relative radius difference exceeds limit.
Description | During the start-up, the channel parameters were checked and it was found that the relative radius difference P-CHAN-00172 is greater than the permissible value of 500.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | During start-up, in case of conflict, the absolute radius difference P-CHAN-00172 is set to 500 [0.1%] and the start-up is continued.
Parameter | %1: | Error value [0.1 µm or 0.0001°]
%2: | Corrected value [0.1 µm or 0.0001°]
Error type | 2, Error message by data transfer from parameter list into control device.