# ID 150051

Index of continuous jog feed rate illegal.
Description | CNC is in manual operation mode and in ENABLED state. This message is issued because the CNC has been instructed to extract the movement velocity value in continuous jog mode (P-AXIS-00077) from the axis parameter data set. It is possible to parametrize different values for the feed rate within the axis parameter data set, and therefore the used feed rate is selected by a index.

When the CNC accepts the data, it detects that no entry in axis parameter data set exists for the specified index.

Response | Class | 1 | Warning The active motion velocity for continuous jog mode at this time is maintained.
Solution | Class | 1 | Command other index at activation of continuous jog mode or Add an entry to the axis parameter data set for P-AXIS-00077 under the corresponding index.
Parameter | %1: | Current value [-]
Index of motion velocity for continuous jog mode for which no entry exists in the axis parameter data set.
Error type | -