# ACS movement limits

These parameters defines the axis-specific movement range in manual mode. In contrast to the offset limits P-AXIS-00137 and P-AXIS-00138, these values are always absolute values which affect the level of the axis coordinates. The adjustable minimum and maximum values are determined by the software limit switches.

Absolute motion limits in manual mode

## Additional information

- Absolute positive ACS movement limit (P-AXIS-00493)
- Absolute negative ACS movement limit (P-AXIS-00492)
- Effect of feedhold control signals (P-AXIS-00529)