# Inner diameter with four points and obstacle

After positioning above the spigot, the touch probe measures along the X and Y axes both in the positive and negative directions after it was again pre-positioned. The touch probe must be positioned as centrally as possible above the spigot either manually or in automatic mode.

Inner diameter with four points and obstacle

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables