# ID 70459

Position overflow in axis forward transformation.
Description | The result of the axis specific forward transformation (conversion of drive position to interpolator position) is larger than the maximum representable position. Possible reasons are: Wrong parametrization of the transformation Activation of the transformation at an inappropriate location
Response | Class | 5 | Error message output, transformation is disabled.
Solution | Class | 6 | Check transformation parameters Check activation position
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Identifier of the axis-specific transformation (P-AXIS-00381)
%3: | Error value [0.1 µm or 0.0001°]
Input position of axis specific transformation
%4: | Limit value [0.1 µm or 0.0001°]
Maximum possible output position
Error type | -