# ID 13245

Velocity for measuring (@P5) is wrong.
Description | The positioning velocity is defined wrong: The measuring feed rate must be greater than 0.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check parameter setting and correct input parameters for the measuring velocity.
Parameter | %1: | Current value
Parameterized measuring velocity
%2: | Lower limit value
Error type | 1, Error message from NC program.