# ID 20577

No longitudinal turning axis configured for cutter radius compensation.
Description | When the tool offsets are accepted with active cutter radius compensation (CRC) for turning tools, the system detects that neither of the plane axes is configured as face turning axis P-AXIS-00015.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | For lathes in the axis parameter list, one of the plane axes (first or second main axis) must be configured as a face turning axis P-AXIS-00015.
Parameter | %1: | Current value [-]
Axis mode of the axis
%2: | Expected value [-]
Number of the "face turning axis"
%3: | Logical axis number [-]
%4: | Logical axis number[-]
Error type | 1, Error message from NC program.