# ID 20430

Channel parameters: Number of groups exceeds maximum limit.
Description | During start-up, the check of the channel parameters detects that the total number of axes groups P-CHAN-00023 exceeds the permissible value range.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | During start-up in case of conflict the total number of axes groups is set to the maximum permissible limit value and the start-up is continued. Note: Possibly not the complete number of configured axes groups of the channel parameter list is available after start-up in the channel!

At the moment in NC channel only one axes group (index 0) is permissible.

Parameter | %1: | Current value [-]
Total number of axis groups P-CHAN-00023
%2: | Limit value [-]
Maximum permissible number of axis groups
%3: | Corrected value [-]
Automatically corrected total number of axes groups
Error type | 2, Error message by data transfer from parameter list into control device.