# ID 150104

Inadmissible value for handwheel counter address (P-MANU-00004).
Description | The manual mode parameters are read and interpreted by the CNC. The CNC detects that a value for manual mode parameters P-MANU-00004 exceeds the CNC system internal limit. Parameter P-MANU-00004 indicates the address to which the handwheel counters are sent to the CNC. When this message is displayed, the high-level interface to the PLC was defined as the transfer location (see P-MANU-00003). The HLI interface selected to transfer the handwheel counter reading is defined in parameter P-MANU-00004 .
Response | Class | 3 | Manual mode parameters are not transferred to the CNC.
Solution | Class | 6 | Correct the value for P-MANU-00004, P-MANU-00004 <= the limit value (see parameter 2 of the message). Reinterpret manual mode parameters by restarting CNC system.
Parameter | %1: | Current value [-]
Index of interface to transfer handwheel counter reading to CNC defined in manual mode parameter data record.
%2: | Limit value [-]
Maximal allowed index value.
%3: | Logical identifier of control element [-]
Identifier of logical control element whose parameters caused the message.
Error type | 2, Error message on data transfer of parameter lists to controller.