# ID 110320

Unknown entry in configuration of output telegram.
Description | At start-up of the CNC kernel, the mapping between the values transmitted cyclically or to the drive, and the internal working of the drive and the internal working data of the CNC is made by entries in the axis parameter list. In one of these entries an unknown value was detected.

In the following example either value 99999 in entry antr.terminal.out[1].signal_nr or value XXXXXX in entry antr.terminal.out[1].nc_ref is invalid.

Example:

antr.terminal.out[1].signal_nr 99999
antr.terminal.out[1].signal_len 2
antr.terminal.out[1].nc_ref XXXXXX

Response | Class | 3 | Error message output, erroneous entry is ignored.
Solution | Class | 6 | Correct invalid entry in the parameter list.
Parameter | %1: | Current value [-]
P-AXIS-00020
%2: | Current value [-]
P-AXIS-00016
%3: | Logical axis number [-]
Index of the invalid entry, in the above example 1.
%4: | Current value [-]
Signal number of the faulty entry, in the above example 99999.
%5: | Current value [-]
Signal name of the faulty entry, in the above example XXXXXX.
Error type | -