# ID 110301

Change of resolution numerator requires a restart.
Description | The parameter P-AXIS-00234 for path resolution numerator of axis cannot be changed while CNC kernel is running. The new numerator value is not transferred, the previous numerator value remains valid.
Response | Class | 0 | None.
Solution | Class | 0 | Change numerator P-AXIS-00234 in configuration mode or when the CNC is inactive.
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis.
%2: |
Current value of P-AXIS-00234.
%3: |
Corrected value of P-AXIS-00234.
Error type | -