# Measure angle in Z axis (A axis)

After positioning, the touch probe measures in the direction of the Y axis. The touch probe must be positioned as centrally as possible at measuring depth at the first measuring point either manually or in automatic mode.

The calculated angle corresponds to the twist of the workpiece about the X axis in relation to the Z axis.

Measure angle in Z axis (A axis)

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables