# Process (internal cycle)

The internal cycle process can be described as follows:

1. Pre-position in Z.
2. Measure in X axis.
3. Clearance in X at starting point.
4. Move back in Z to starting position.
5. Position in X, Y and Z above the 2nd
6. Pre-position in X direction.
7. Pre-position in Z direction.
8. Measure in X+ direction.
9. Clearance in X- direction.
10. Move back to Z start.
11. Move back to X start.
12. Then follow measurements in X+, Y- and Y+
13. Description of selected zero offset.