# Angle measurement between point in Y and pin (C axis)

Position the touch probe in front of the required surface above the workpiece, either manually or in automatic mode, before the cycle is started.

If no C axis is configured, call the cycle without transferring @P7. The twist in C can be manually transferred to the related zero offset by evaluating the output variables in the post-program.

Measure angle between point in Y and spigot (C axis)

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables