# ID 1599

Not enough path in motion block for position controlled stop.
Description | After activation of measurement signal via measuring probe, residual path P-CHAN-00030 defined in channel parameter list is reduced with active function edge banding. The residual path available of current active channel block at this moment must be greater than P-CHAN-00030. Depending on setting of P-CHAN-00029 the residual path is reduced by one or more blocks. Braking distance after activation of probing sensor depends on dynamic settings in axis machine data!

For further information, see PROG// Section: Edge banding.

Response | Class | 6 | Program abort.
Solution | Class | 7 | Check whether there is sufficient block residual path available in the NC program after activating the measuring probe. Increase residual path or, if possible, reduce the value of channel parameter P-CHAN-00030.
Parameter | %1: | Expected value [0.1 µm or 0.0001°]
Current braking distance.
%2: | Current value [0.1 µm or 0.0001°]
Current residual distance in the block.
Error type | 1, Error message from NC program.