# ID 20940

Programmed spindle speed is out of speed ranges.
Description | In the channel parameters, spindle gear changes are enabled (P-CHAN-00052). The programmed spindle speed cannot be covered by any of the speed ranges or gear stages defined in the channel parameters for this spindle (P-CHAN-00058, P-CHAN-00055).
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the NC program. Adapt the programmed spindle speed in the way, that it is within the defined speed ranges of the spindle. Alternatively, if it is (mechanically) possible to redefine the speed ranges in the channel parameters (P-CHAN-00058, P-CHAN-00055) so that the programmed spindle speeds can be executed.
Parameter | %1: | Current value [-]
Programmed spindle speed
Error type | 1, Error message from NC program.