# Preparing the calculation cycle

There is a programming example to execute the calculation for every available kinematic without automatic measurement. They are:

- SysCalibFit009V0Demo.nc
- SysCalibFit057V0Demo.nc
- SysCalibFit058V0Demo.nc
- SysCalibFit059V0Demo.nc
- SysCalibFit060V0Demo.nc
- SysCalibFit080V0Demo.nc
- SysCalibFit090V0Demo.nc
- SysCalibFit090V2Demo.nc

## Additional information

- Adapting the output file
- Adapting the output format
- Adapting the limit for deviation
- Initialising the kinematic calculation
- Entering measurement results
- Kinematic-specific changes