# Valid deceleration ramp at FEEDHOLD (P-CHAN-00097)

P-CHAN-00097 | Valid deceleration ramp at FEEDHOLD
Description | This parameter defines the deceleration ramp used when FEEDHOLD is active.
Parameter | use_drive_curr_limit
Data type | BOOLEAN
Data range | 0: When FEEDHOLD occurs, deceleration takes place using the currently valid deceleration rate. 1: With FEEDHOLD, the parameterised deceleration in P-AXIS-00024 and the ramp time set in P-AXIS-00081 are used for deceleration. If these two parameters are not set, deceleration takes place at the current deceleration value (P-AXIS-00053).
Dimension | ----
Default value | 0
Remarks |