# Distance between interpolation points on the second master axis (P-COMP-00033)

P-COMP-00033 | Distance between the interpolation points on the second master axis
Description | The parameter defines the interval between two interpolation points for the first master axis if both master axes use a different grid (P-COMP-00031(grid) = RECTANGULAR).
Parameter | kw.crosscomp2.interval2
Data type | UNS32
Data range | 0 < interval2 < MAX(UNS32)
Axis types | T, R, S
Dimension | T: 0.1 µm or increments | R,S: 0.0001° or increments
Default value | 0
Remarks |