# ID 110466

Measuring method not validated. Only one method may be selected.
Description | In addition to the parameter P-AXIS-00330, one of the parameters P-AXIS-00269,P-AXIS-00117, P-AXIS-00115, P-AXIS-00116 or P-AXIS-00257 has been enabled. If @@P-AXIS-00330 is not enabled, no other measurement method can be enabled.
Response | Class | 1 | Error message output, P-AXIS-00269, P-AXIS-00117, P-AXIS-00115, P-AXIS-00116 and P-AXIS-00257 are set to zero (nil).
Solution | Class | 1 | Configure measurement method correctly.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Value of P-AXIS-00330.
Error type | 2, Error message by data transfer from parameter list into control device.