# ID 60158

Positive software limit switch exceeded.
Description | The positive software limit switch will be exceeded. Software limit switch monitoring is done based on the current position and speed of the axis, taking into account the braking distance of the software limit switches. If the axis passes over the software limit switch, the error message is output.

The position of the software limit switch is defined by parameter P-AXIS-00178 and can be changed in the NC program by G99.

See also

[PROG// Section: Setting the positive software limit switch (G99)]

[FCT-A2// Section: Program the positive software limit switch].

Response | Class | 7 | Stopping the axis, aborting the NC program.
Solution | Class | 6 |
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [0.1 µm or 0.0001°]
Current axis position.
%3: | Limit value [0.1 µm or 0.0001°]
Position of software limit switch
%4: | Current value [0.1 µm or 0.0001°]
Current axis position + braking distance (=stop position)
Error type | -