# ID 50961

Start position not in workspace..
Description | The start position in manual mode is outside the workspace when workspace and protection area monitoring is active [FCT-C14// Special features in manual mode]. This is not possible with the selected setting of P-CHAN-00442.
Response | Class | 6 | Abrupt stop for all axes.
Solution | Class | 6 | Check the workspace, check P-CHAN-00442. Set the Suppress error output from workspace monitoring in manual mode control unit to move backward in the workspace in manual mode.
Parameter | %1: | Identification number [-]
ID of the workspace affected
%2: | Current value [-]
Bit identifier of the affected axes
%3 | Error value [0.1 10^-3 mm or ø]
3-dimensional output of positions
Error type | 1, Error message from NC program.