# ID 60138

Technology function for spindle not permitted, if spindle not present.
Description | An attempt was made to output a technology function (M/H/S function) on the spindle axis although the spindle axis was previously released due to an axis exchange command. Example: .. N1000 S[PUTAX] N1100 S100 (Error ! )

N1200 X1000

..

In the above example program, an error message is issued in line N1100 because the spindle axis was issued by the S[PUTAX] command in line N1000 at the time the S function was programmed.

See also [PROG// Section: Releasing/requesting spindle axes]

[FCT-C1// Section: Spindle M functions].

Response | Class | 6 | Movement stop., Abort the NC program.Movement stop.
Solution | Class | 6 | Change the NC program.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
Error type | 1, Error message from NC program.