# Resolution of linear axes (P-CHAN-00034)

P-CHAN-00034 | Resolution of linear axes
Description | This value of this parameter represents the conversion factor between the motion paths or positions programmed in the NC program and the internal representation of positional values for linear axes.
Parameter | lin_aufloes
Data type | REAL64
Data range | 0 < lin_aufloes < MAX(REAL64)
Dimension | ----
Default value | 10000
Remarks | Not to be confused with the resolution of the drive encoder P-AXIS-00234/P-AXIS-00235. As of CNC Build V2.11.2026.09 P-CHAN-00315 replaces the parameters lin_aufloes, rund_aufloes and spind_aufloes (P-CHAN-00034, P-CHAN-00035 and P-CHAN-00036). It is recommended to use only P-CHAN-00315 as of this CNC Build.

Parameterisation example: All translatory axes are specified in the dimension 'millimeter' [mm] in the NC program.

lin_aufloes 10000

Internal representation in [0.1 µm] | Typical value for liner resolution | Programmed value in the NC program in [mm]
10 000 [0.1µm] | 10 000 | 1 [mm]