# ID 21889

Feedrate is out of permissible value range.
Description | The programmed feedrate is outside of the permitted range.
Response | Class | 2 | Reset of the NC channel.
Solution | Class | 3 | Correct the feedrate to a valid value.
Parameter | %1: | Lower limit value [-]
Minimal permitted value.
%2: | Upper limit value [-]
Maximum value that the feed can take.
Error type | 1, Error message from NC program.