# ID 60102

Warning level of axis velocity exceeded.
Description | The maximum axis velocity set in the axis parameter list (P-AXIS-00212) was exceeded by at least 5 percent. This error message is used for diagnosis of the dynamic look-ahead and is only output if the NC kernel is parameterised accordingly.
Response | Class | 1 | None
Solution | Class | 1 |
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [1µm/s or 0.001°/s]
Current command velocity of the axis.
%3: | Limit value [1µm/s or 0.001°/s]
Maximum permissible velocity of the axis (P-AXIS-00212).
%4: | Current value [-]
Ratio of current velocity to maximum permissible axis velocity (absolute value).
%5: | Limit value[-]
Maximum tolerable ratio of actual velocity to maximum permissible velocity.
Error type | 1, Error message from NC program.