# Dead time (P-AXIS-00194)

P-AXIS-00194 | Dead time for drive simulation
Description | The parameter defines the dead time.
Parameter | antr.simu.totzeit
Data type | UNS32
Data range | 5 (Maximum possible dead time, application-specific) ≥ totzeit ≥ 0
Axis types | T, R, S
Dimension | T: Number of interpolation cycles * | R,S: Number of interpolation cycles *
Default value | 0
Drive types | Simulation
Remarks | * The dead time is defined as a multiple of cycle time TAb of geometry data processing of the NC kernel.