# Output of additional error information (P-AXIS-00632)

P-AXIS-00632 | Output of additional error information (filtering of axis error messages)
Description | This text is forwarded transparently via the CNC_ERROR_INFO data structure if the filter condition applies, i.e. users have a possibility of conditionally also including additional error information in the output.
Parameter | error_filter[i].conditional_output where i = 0 ... 3 (maximum number of filters, application-specific)
Data type | STRING
Data range | Maximum of 32 characters
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | *
Remarks | * Note: The default value of variables is a blank string.