# ID 110489

Invalid value for parameter P-AXIS-00353 is corrected.
Description | The axis was parameterised as an edge banding axis antr.edge_bending_input_nbr (P-AXIS-00098) and an invalid value was specified for the edge banding input to be used at the drive (parameter P-AXIS-00353).
Response | Class | 1 | Warning and correction of parameter. P-AXIS-00353 is corrected to 1
Solution | Class | 1 | In the axis parameter list, assign to parameter P-AXIS-00353 a value valid for the drive type used (P-AXIS-00020). In the actuator, the latch function must be assigned to the digital input used.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [-]
%3: | Lower limit value [-]
%4: | Upper limit value [-]
%5: | Corrected value [-]
Error type | 2, Error message by data transfer from parameter list into control device.