# ID 21257

Multiple use of the same axis index.
Description | Within the axis exchange command, an attempt is made to exchange different axes for the same index (space) in the channel.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the axis exchange command. Assign different free indices (places) of the channel to the corresponding axes.
Parameter | %1: | Error value [-]
Index of the axes in the axis exchange command. [CHAN//section: Configuration of the path axes]
Error type | 1, Error message from NC program.