# ID 110528

The parametrized controller deadband is bigger than the position window.
Description | The set up position controller deadband (P-AXIS-00395) is bigger than the position window (P-AXIS-00236) set for the axis.
Response | Class | 1 | Error message output, P-AXIS-00395 is limited to the value of P-AXIS-00236.
Solution | Class | 1 | Either resize P-AXIS-00395 or enlarge P-AXIS-00236.
Parameter | %1: | Logical axis number [-]
Log. Axis number (see also P-AXIS-00016).
%2: | Error value [0.1 µm or 0,0001°]
Value of P-AXIS-00395.
%3: | Limit value [0.1 µm or 0.0001°]
Value of P-AXIS-00236.
%4: | Corrected value [0.1 µm or 0.0001°]
Corrected value of P-AXIS-00395.
Error type | 2, Error message by data transfer from parameter list into control device.