# ID 13126

The machining mode for threads (@P13) is defined incorrectly.
Description | Error in the definition of parameter @P13 for the machining mode. Permissible value for @P13 are: 0 - thread tapping to final drilling depth (default) 1 - chip breaking 2 - chip evacuation
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and correct definition of thread type @P10.
Error type | Error message from NC cycle