# ID 110228

Logical axis number in compensation data list and in command PDU not equal.
Description | CNC is commanded to parametrise an axis with values from a specified list. This message is output because the number of the logical axis in the list is not the same as the number of the axis.
Response | Class | 3 | Abort interpretation of the list.
Solution | Class | 7 | Check which list is to be used to parameterise the axis. Possibly change change the number of the logical axis in the list or use a different list.
Parameter | %1: | Current value [-]
Number of a logical axis. This number comes from the list that was to be interpreted.
%2: | Expected value [-]
Number of logical axis which is to be parametrised with the values contained in list.
Error type | -