# Select specific manufacturer-specific procedures for drive controllers (P-AXIS-00535)

P-AXIS-00535 | Select specific manufacturer-specific procedures for drive controllers
Description | Many drive controllers do not always conform completely to the interface specifications. In conjunction with P-AXIS-00536 this parameter can activate manufacturer- and device-specific special procedures to still operate the drive controller in the CNC.
Parameter | kenngr.vendor_id
Data type | UNS32
Data range | 0: No special procedures active 100: Specify the activated special procedures in P-AXIS-00536 in the form of a bit string. The purpose of values 1 to 9 are to enable a manufacturer-specific set of special procedures and they only exist for the purpose of downward compatibility.
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | ----
Remarks |