# ID 270071

An error message could not be written to the HLI (axis interface).
Description | The PLC reported receipt of the error messages at the HLI; however, it executes them in a job that is too slow. As a result, not all error messages can be sent to the PLC. The information is incomplete. Reading error messages should be executed in a faster job to ensure that all error messages can be received.
Response | Class | 3 | Creating a new error message
Solution | Class | 7 | Increase the priority of the PLC task and the cycle time.
Parameter | %1: | Current value [-]
Error ID of the error message that was not transmitted
%2: | Logical axis number [-]
Error type | -