# ID 20634

No face turning axis is configured in the actual plane at G96.
Description | With the selection of constant cutting speed (G96) it is detected, that not any of the plane axes is configured as face turning axis P-AXIS-00015.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | For lathes in the axis parameter list, one of the plane axes (first or second main axis) must be configured as face turning axis P-AXIS-00015.
Error type | 1, Error message from NC program.