# ID 110581

Changing of P-AXIS-00511 requires restart of the control.
Description | The value P-AXIS-00511 is to be changed by updating a parameter list; this is only permitted if the "ALLOW_RESOLUTION_CHANGE" bit is set in P-AXIS-00015.
Response | Class | 0 | Error message output, new value is not adopted.
Solution | Class | 0 | In parameter P-AXIS-00015 set the "ALLOW_RESOLUTION_CHANGE" bit or change P-AXIS-00511 by controller restart.
Parameter | %1: |
Axis number
%2: |
Set value of P-AXIS-00511.
%3: |
Corrected (old) value of P-AXIS-00511.
Error type | -