# ID 50909

Error in calculation / preparation of shift value.
Description | In connection with the #SHIFT functionality (*) the iterative calculation algorithm was unable to calculate a valid shift value with the current conditions due to the programmed geometry, the technology parameters and the measurement.
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Please contact the control manufacturer.
Parameter | %1: | Block number [-]
Block number of the current block described
%2: | Line number in file [-]
Line number of the current block described
%3: | Current value [-]
Block type of the current block described
Error type | 1, Error message from NC program.