# ID 120681

Invalid superimposed movement with independent axis.
Description | With active tube profile machining ((#CYL[EDGES=...]), an independent axis was programmed which is an input axis of the tube transformation. Crossing the profile rounding of the tube leads to invalid superimposed movement. Programming of independent movement is only allowed on plane sections of profile.
Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Check and correct the NC program.
Error type | 1, Error message from NC program.