# ID 110298

Changing sign of actual value requires a restart.
Description | The parameter P-AXIS-00230 that indicates the sign of current value cannot be changed while CNC kernel is running. The modified sign value is not transferred, the previous sign value remains valid.
Response | Class | 0 | None.
Solution | Class | 0 | Change the sign P-AXIS-00230 in configuration mode or when the CNC is inactive.
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis.
%2: |
Current value of P-AXIS-00230.
%3: |
Corrected value of P-AXIS-00230.
Error type | -