# ID 110086

Implausible contour resolution.
Description | The denominator of the path resolution P-AXIS-00233 of the measuring system was zero (nil). A value unequal to zero (nil) must be specified. The path resolution is specified as factor P-AXIS-00234 / P-AXIS-00233 in increments per 0.1 µm or per 0.0001°.
Response | Class | 1 | Initialization of resolution with default value
Solution | Class | 1 | Correction of denominator in the parameter list
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [-]
P-AXIS-00233
%3: | Corrected value [-]
P-AXIS-00233
Error type | 2, Error message by data transfer from parameter list into control device.