# ID 70169

No release for the drive amplifier.
Description | A Lightbus drive is to be be moved although release of the drive amplifier is not set.
Response | Class | 8 | Open-loop controlled stop of axis affected
Solution | Class | 6 | Activate the switch for the drive amplifier release
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis, see P-AXIS-00016
%2: | Current value [-]
State of drive (state byte 3)
Error type | 11, Error message from position controller.