# ID 50686

Homing of axis not possible since homing is disabled in axis parameters.
Description | The axis cannot be homed, since homing is deactivated (see axis parameter homing_type P-AXIS-00299).
Response | Class | 6 | Error message output, abort NC program
Solution | Class | 6 | Correct NC program. If the axis does not have an absolute measuring system, change parameter P-AXIS-00299.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Drive type [-]
Drive type P-AXIS-00020 of the axis
%3: | Current value [-]
Current value of the parameter P-AXIS-00299
Error type | 1, Error message from NC program.