# ID 120215

Stroke of probe is 0 in axis data.
Description | If the measuring function G100 is used, certain measurement types can check and include the stroke of the measuring probe P-AXIS-00086 during the measuring travel. In this case, this parameter must be assigned in the MDS. The path velocity is then reduced during the measuring travel to such an extent that it can be stopped within the probe stroke after the measuring probe has responded.

For detailed information on measuring function G100, see
FCT-C4// Section: Introduction
[PROG// Section: Measuring functions].

Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Set MDS parameter P-AXIS-00086 according to the permissible stroke of the measuring probe.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
Error type | 2, Error message by data transfer from parameter list into control device.