# ID 70225

During active velocity monitoring maximum speed was exceeded.
Description | The maximum permissible actual velocity P-AXIS-00311 was exceeded during active velocity monitoring.
Response | Class | 7 |
Solution | Class | 6 | Check actual velocity or maximum permissible actual velocity P-AXIS-00311 and perform NC reset.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [1µm/s or 0.001°/s]
Current velocity value.
%3: | Limit value [1µm/s or 0.001°/s]
Maximum permissible actual velocity P-AXIS-00311.
Error type | 11, Error message from position controller.