# ID 50454

No clear of backward storage during backward on path possible.
Description | In the backward motion function on the path, the signal in the bahn_mc_control.backward_storage_off.command_w control unit was activated to clear the storage for backward motion. This is not possible when backward motion is active. The backward motion storage is not cleared.

For more information on backward motion [FCT-C7// Section : Forward/backward motion on the path]

Response | Class | 1 | None.
Solution | Class | 1 | Do not set the PLC signal bahn_mc_control.backward_storage_off.command_w when path motion is active.
Error type | -