# ID 110064

All axis have to have different axis numbers.
Description | Two axes in the system have been assigned the same logical axis number P-AXIS-00016. This is not permitted. The data transfer for the second axis with the same logical axis number is rejected.
Response | Class | 1 | None.
Solution | Class | 1 | All the axes in the system have different logical axis numbers P-AXIS-00016 .
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current logical axis number.
%3: | Corrected value [-]
Corrected logical axis number P-AXIS-00016.
Error type | 2, Error message by data transfer from parameter list into control device.